**PA 2 - B Requirements**

* Transmit messages from A to B without waiting for ACKs.
* Track the number of message simultaneously in transit.
* When there are 8 messages in transit, start buffering.
* When there are 50 messages in the buffer, start dropping.